**Project Arduino**

|  |  |  |
| --- | --- | --- |
| Screen | Also known as | Arduino pin |
| GND | earth | GND |
| Vdd | supply voltage | 5v |
| SCK | serial clock, OLED\_CLK | 13 |
| SDA | serial data, OLED\_MOSI | 11 |
| RES | Reset, OLED\_RESET | 10 |
| D/C | data/command, DC, OLED\_DC | 9 |
| CS | chip select, OLED\_CS | GND |

|  |  |
| --- | --- |
| Module | Arduino Uno |
| Vcc | Breadboard 5V |
| GND | Breadboard GND |
| STB | 5 |
| CLK | 6 |
| DIO | 7 |

|  |  |
| --- | --- |
| Rotary Encoder | Arduino Uno |
| Outer Pin 1 | 2 |
| Middle Pin | GND (or breadboard GND) |
| Outer Pin 2 | 3 |

|  |  |
| --- | --- |
| Servo | Arduino Uno |
| Black | Breadboard GND |
| Red | 5v |
| White | 8 |